Open topic with navigation

TIBCO® Managed File Transfer Platform Server for z/OS 8.1.0

# FUSNODE

You can use the FUSNODE exec to display information on enabled NODE definitions.

## Required Parameters

This exec does not has required parameters.

## Optional Parameters

The following table lists the optional parameters of the FUSSCMD exec:

Parameter | Description
--- | ---
CONFIG | CFG | Defines the configuration file used by the FUSNODE exec. If this parameter is not defined, the Platform Server REXX uses the default configuration.
NODE | Defines the NODE definition on which detailed information is to be displayed. If this parameter is not specified, a list of enabled NODE definitions is displayed.
INIHOLD | Modifies the defined NODE definition to turn on the Initiator Hold flag. This indicates that initiator requests to this node will not be dispatched. The NODE parameter must be defined.
INITREL | Modifies the defined NODE definition to reset the Initiator Hold flag. This indicates that Initiator requests to this node will be dispatched. The NODE parameter must be defined.
RESPHOLD | Modifies the defined NODE definition to turn on the Responder Hold flag. This indicates that the responder requests from this node will be rejected with a recoverable error. The NODE parameter must be defined.
RESPREL | Modifies the defined NODE definition to reset the Responder Hold flag. This indicates that the responder requests from this node will be accepted. The NODE parameter must be defined.

## Return Codes

The following table lists the return codes of the FUSNODE exec:

Return Code | Description
--- | ---
`0` | Indicates that the Platform Server has successfully displayed the message.
`5` | Indicates that the NODE was not enabled.
Any other return code | Indicates a network error occurred when processing a request.

## Example

The following is an example of using the FUSNODE exec to display information on enabled NODE definitions:

    FUSNODE N=TESTNODE

The output of this example is as follows:

    ONode Name...........= TESTNODE
    IP Address..........= 192.192.100.10
    IP.Port.............= 46464
    STATUS..............= Normal
    SSL.................= No
    Protocol............= *Default
    Parallel............= YES
    Cont.Winners........= 00005
    Cont.Losers.........= 00005
    Encrypt.............= NONE
    retncode===> 0
    utput

Copyright © 2003-2021. TIBCO Software Inc. All Rights Reserved.