Open topic with navigation

TIBCO® Managed File Transfer Platform Server for z/OS 8.1.0

# JCL Requirements

STEPLIB must include the load library that contains the Platform Server load modules:

Statement | Description
--- | ---
VTAMTRAC | An optional DD statement. You must define this statement when using SNA to communicate with the Platform Server started task and API_SERVER_TRACE_FLAG is set to `API_SERVER_TRACE_YES`. Output from this DD is typically sent to SYSOUT.
TCPTRAC | An optional DD statement. You must define this statement when using TCP (IPADDR or IP Name) to communicate with the Platform Server started task and API_SERVER_TRACE_FLAG is set to `API_SERVER_TRACE_YES`. Output from this DD is typically sent to SYSOUT.
SYSPRINT | DD statement. The name used for this DD statement can be any valid DD name. However, the API calling program must have an OPEN DCB for this DD name with the following characteristics: RECFM=`FBA` LRECL=`133` MACRF=`PM`
AUDPATH1/2 | Two DD statements. These two DD Statements are required under the following circumstances: The server type is PCCALL. The server function is Transfer Status.

Copyright © 2003-2021. TIBCO Software Inc. All Rights Reserved.