Open topic with navigation

ibi™ Open Data Hub for Mainframe Connectors 1.0.8

# IP Port Number Requirements

The install process prompts for two IP port numbers: the TCP lListener and HTTP listener. It also uses the next two consecutive ports after the supplied HTTP listener port for FDS use. This results in a total of four IP ports.

The supplied IP port numbers must be above the IANA registered well-known reserve range (numbers under 1024) and not over the maximum legal number (65535). Additionally, do not use IP port numbers already being used by other applications or products. Netstat, or netstat like commands, should reveal what actual ports are in use.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

ibi™ Open Data Hub for Mainframe Connectors

Copyright © 2021-2025. Cloud Software Group, Inc. All Rights Reserved.