Open topic with navigation

TIBCO Rendezvous® 8.7.0

# Fault Tolerance Road Map

For a complete discussion of concepts and operating principles, see Fault Tolerance Concepts on page 169 in TIBCO Rendezvous Concepts.

For suggestions to help you design programs using fault tolerance features, see Fault Tolerance Programming on page 187 in TIBCO Rendezvous Concepts.

For step-by-step hints for implementing fault-tolerant systems, see Developing Fault-Tolerant Programs on page 199 in TIBCO Rendezvous Concepts.

Fault tolerance software uses advisory messages to inform programs of status changes. For details, see Fault Tolerance (RVFT) Advisory Messages on page 285 in TIBCO Rendezvous Concepts.

If your application distributes fault-tolerant processes across network boundaries, you must configure the Rendezvous routing daemons to exchange `_RVFT` administrative messages. For details, see Fault Tolerance on page 385 in TIBCO Rendezvous Administration, and discuss with your network administrator.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2023. Cloud Software Group, Inc. All Rights Reserved.