Open topic with navigation

TIBCO Rendezvous® 8.7.0

# DISABLING_MEMBER

Advisory

## Subject Name Syntax

    _RV.ERROR.RVFT.DISABLING_MEMBER.group

## Purpose

Rendezvous fault tolerance software sometimes detects problems that make a fault tolerance member unable to function. It automatically deactivates the affected member, disables it (by setting its weight to zero), and generates this error advisory message.

## Remarks

Only the disabled member presents this advisory.

The `RVADV_DESC` field always contains `NULL`.

This advisory indicates that Rendezvous fault tolerance software cannot allocate memory, publish a message or set a timer. In most cases, the primary cause is insufficient memory.

In some cases, memory is so scarce that the disabled member is unable to process the advisory message, nor even relay the advisory message to `stderr`.

For a complete discussion, see Disabling a Member.

## Remedy

The most reliable remedy is to arrange for the process to exit gracefully, and then restart the member. In the meantime, the disabled process is replaced by another member (presuming that other members are running). Be certain to investigate and correct the cause of the resource problem.

## Message Fields

Field Name | Description
`RVADV_DESC` | A string describing the specific situation of this advisory. This field has datatype `TIBRVMSG_STRING.`

## See Also

Fault Tolerance Concepts

Disabling a Member

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2023. Cloud Software Group, Inc. All Rights Reserved.