Open topic with navigation

TIBCO Rendezvous® 8.7.0

# DELIVERY.NO_RESPONSE

Advisory

## Subject Name Syntax

    _RV.WARN.RVCM.DELIVERY.NO_RESPONSE.name

## Purpose

A sender presents this advisory when a listener does not confirm certified messages.

## Remarks

The advisory repeats at a regular interval until the sender receives a delivery confirmation from the listener.

When several certified listeners are unresponsive, the sender presents a separate advisory for each one.

The `name` element is the name of the unresponsive listener. The listener name can span several elements, so the wildcard character `">"` (rather than `"*"`) is the correct way to match all subjects in this position.

## Message Fields

Field Name | Description
`listener` | The name of the listener that has not confirmed message delivery. It is identical to the `name` element. This field has datatype `TIBRVMSG_STRING.`

## Diagnosis

`DELIVERY.NO_RESPONSE` advisories can indicate any of these difficulties:

| • | The physical network is unreliable.

| • | The receiving program has terminated or is unstable.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2023. Cloud Software Group, Inc. All Rights Reserved.