Open topic with navigation

TIBCO Rendezvous® 8.7.0

# rvperfm

Command

## Syntax

    rvperfm  [-service service ]
             [-network network ]
             [-daemon daemon ]
             [-subject subject ]
             [-inbox]
             [-auto]
             [-non-vectored]
             [-terse]
             [-messages m ]
             [-size size ]
             [-interval interval ]
             [-batch batch_size ]
             [-cm]
             [-cm-name name ]
             [-cm-ledger filename ]
             [-cm-sync]
             [-h]

## Purpose

`rvperfm` coordinates the tasks of measuring network performance. It sends messages to the network, and reports statistics to `stdout`.

## Remarks

In single mode (without the flag `-auto`), `rvperfm` sends one run of messages, and then exits.

In automatic mode (with the flag `-auto`), `rvperfm` sends several runs of messages, adjusting the batch size and interval parameters to empirically determine the combination that yields maximum network throughput. After it finds the optimal settings, it exits; the parameters and report of the final run reflect optimal network performance. For details, see Automatic Mode—Binary Search.

## Outline

Each run consists of these steps:

Procedure

| 1. | Dynamically discover the available `rvperfs` processes; output a list of participating instances. In the discovery step, `rvperfm` polls for listeners, and waits 3 seconds for ready signals from `rvperfs` processes; then it continues to the next step.

| 2. | Send the run of messages.

| 3. | Output statistics that measure the performance of the sender.

| 4. | Output statistics that measure the performance of each receiver (if any).

| 5. | Output a summary of error advisories pertaining to the sender.

## Collision

When two instances of `rvperfm` (simultaneously) attempt to use the same subject, service and network, at least one of them detects the collision and exits immediately.

Simultaneous instances that differ in subject or service (or both) do not constitute a collision. Such processes can coexist.

Parameter | Description
`-service` `service` | `service` is the service name or UDP port number that defines the service group. See Service Selection. If you do not specify the `-service` parameter, the default value is `7599`.
`-network` `network` | `network` narrows the service group by selecting a local network by network name or IP network number (when the host computer has multiple network interfaces). It can also specify multicast addresses. See Network Selection. If you do not specify the `-network` parameter, the default value is the multicast address`";225.9.9.9"`. On operating systems that do not support multicast addressing, you must supply a valid broadcast network address.
`-daemon` `daemon` | The `-daemon` parameter instructs the program about how and where to find `rvd` and establish communication. See Daemon Client Socket—Establishing Connections. You can specify a daemon on a remote computer. For details, see Remote Daemon. However, the program cannot start a remote daemon automatically—you must start it manually on the remote computer. If you do not specify the `-daemon` parameter, the program finds the local daemon on TCP socket `7500`.
`-subject` `subject` | `rvperfm` sends messages to this subject name. If you specify neither `-subject` nor `-inbox`, then the program uses `_perf` as a prefix to construct broadcast subjects.
`-inbox` | `rvperfm` sends point-to-point messages `rvperfm` probes the network to discover available instances of `rvperfs`. The first instance to respond becomes the sole receiver—`rvperfm` sends point-to-point messages only to an inbox in that process instance. (Since `rvperfm` uses broadcast subjects for the initial discovery phase, it is not a contradiction to specify both `-inbox` and `-subject` parameters. When both parameters are present, `-inbox` determines the sending behavior.)
`-auto` | When present, `rvperfm` operates in automatic mode, sending several runs of messages to automatically determine the optimal batch size and interval parameters for the network. When absent, `rvperfm` operates in single mode, sending only one run of messages. See also, Automatic Mode—Binary Search.
`-non-vectored` | When present, `rvperfm` sends individual messages. When absent, `rvperfm` sends each batch of messages using a single vector call.
`-terse` | When present, suppress most reporting and simplify the final report. The terse final report contains one line per receiver (`rvperfs`). Each line is a comma-separated list of the following values: send message rate, received message rate, send byte rate, received byte rate, elapsed send time, elapsed receiver time, receiver SlowConsumer, receiver DataLoss, messages sent, send size, batch interval, batch size, reply name For descriptions of these values, see -reliability time.
`-messages` `m` | `rvperfm` sends `m` messages per run. If not present, the default is 10000 messages per run.
`-size` `size` | `rvperfm` sends messages with `size` bytes of payload data. Use this size to model application data rates. This size does not include message header data nor packet overhead, so computing the network byte transfer rate from this size results in an slight underestimate of the actual throughput. If not present, the default is 256 payload bytes in each message.
`-interval` `pause` | `rvperfm` sends messages in batches, waiting for `pause` seconds between the end of one batch and the start of the next batch. When absent, the default pause is zero seconds. In single mode, `rvperfm` sends the run with this interval. In automatic mode, `rvperfm` sends the first run with this interval, adjusting the parameters in subsequent runs. Warning Change of Units: In earlier releases the value of this parameter was interpreted as milliseconds—now it is a floating point value interpreted as seconds.
`-batch` `batch_size` | `rvperfm` sends messages in batches, with `batch_size` messages in each batch. When absent, the default is 128 messages per batch. To send messages individually, specify 1 as the `batch_size`. In single mode, `rvperfm` sends the run with this batch size. In automatic mode, `rvperfm` sends the first run with this batch size, adjusting the parameters in subsequent runs.
`-cm` | When present, `rvperfm` sends messages with certified delivery features. If `rvperfs` also specifies `-cm`, then the programs establish a certified delivery agreement.
`-cm-name` `name` | When present, `rvperfm` specifies this reusable correspondent name when it enables certified delivery. When `-cm` is present, but `-cm-name` is not, `rvperfm` operates with a non-reusable correspondent name.
`-cm-ledger` `filename` | When present, `rvperfm` uses this ledger file. You must also supply `-cm-name`.
`-cm-sync` | When present, then operations that update the ledger file do not return until the changes are written to the storage medium. You must also supply `-cm-ledger` and `-cm-name`. When absent, the operating system writes ledger file changes to the storage medium asynchronously.
`-h` | When present, output a parameter usage list to `stdout`, and exit immediately.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2023. Cloud Software Group, Inc. All Rights Reserved.