Open topic with navigation

TIBCO Rendezvous® 8.7.0

# Very Large Messages

Rendezvous software can transport very large messages; it divides them into small packets, and places them on the network as quickly as the network can accept them. In some situations, this behavior can overwhelm network capacity; applications can achieve higher throughput by dividing large messages into smaller chunks and regulating the rate at which it sends those chunks. You can use the performance tool to evaluate chunk sizes and send rates for optimal throughput.

This example, sends one message consisting of ten million bytes. Rendezvous software automatically divides the message into packets and sends them. However, this burst of packets might exceed network capacity, resulting in poor throughput:

        sender> rvperfm -size 10000000 -messages 1

In this second example, the application divides the ten million bytes into one thousand smaller messages of ten thousand bytes each, and automatically determines the batch size and interval to regulate the flow for optimal throughput:

        sender> rvperfm -size 10000 -messages 1000 -auto

By varying the `-messages` and `-size` parameters, you can determine the optimal message size for your applications in a specific network. Application developers can use this information to regulate sending rates for improved performance.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2023. Cloud Software Group, Inc. All Rights Reserved.