Open topic with navigation

TIBCO Rendezvous® 8.7.0

# CLIENT.IP_MISMATCH

Advisory

## Subject Name Syntax

    _RV.ERROR.SYSTEM.CLIENT.IP_MISMATCH

## Purpose

A client transport receives this advisory when it reconnects to daemon, and the daemon’s IP address is different from the IP address of the original connection.

## Background

Point-to-point message delivery relies on a transport connection to a daemon with an IP address that remains constant. If a client transport loses connectivity, and reconnects to a daemon with a different address, then that transport cannot support point-to-point connectivity (nor any features that rely on point-to-point connectivity).

## Remarks

Only the specific client transport receives this advisory.

This message is an error, however the daemon does not reject the connection, and the transport continues to support multicast message delivery.

## Message Fields

Field Name | Description
`tport` | The transport ID.
`descr` | The client’s description string.

## Diagnosis

This error can occur in a network architecture that uses virtual IP addresses. The redirector might assign one remote daemon when a transport first connects, but might assign a different daemon when the transport attempts to reconnect. In this situation, transport behavior is undefined.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2023. Cloud Software Group, Inc. All Rights Reserved.