Open topic with navigation

TIBCO Rendezvous® 8.7.0

# Selecting the Network Interface

UNIX

On UNIX platforms with more than one network interface, use `iniftst` to determine the correct interface name.

Windows

On Windows platforms with more than one network interface, it is sometimes difficult to determine the correct interface name. The remainder of this section presents a method to determine it:

Procedure

| 1. | If data capture appears correct, then the remaining steps are not needed. However, if the captured data is all zeroes, then specify a different network interface (using `rvtrace -i`). Only one of the interfaces carries the data that `rvtrace` requires.

| 2. | Install the `WinDump` utility from this URL:

http://www.winpcap.org/windump/install/default.htm

| 3. | Use this command to obtain a list of interface names:

`windump -D`

| 4. | Try each interface until the data appears reasonable.

Consider this example:

    C:\>windump -D
    1.\Device\Packet_{D7308399-80B2-4CA1-A9E6-C90DD74511A8} (EL574ND4 Ethernet Adapter)
    2.\Device\Packet_NdisWanIp (NdisWan Adapter)
    C:\>rvtrace -i \Device\Packet_{D7308399-80B2-4CA1-A9E6-C90DD74511A8}

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2023. Cloud Software Group, Inc. All Rights Reserved.