Open topic with navigation

TIBCO Rendezvous® 8.7.0

# Adapter Start Phase

When the adapter starts, it does these preparatory steps.

1. The adapter reads the configuration file.
2. The adapter contacts the FTL server to get the realm definition.
3. The adapter validates its configuration.
4. If the start phase succeeds in reaching this point, the adapter starts both its FTL side and its Rendezvous side.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2023. Cloud Software Group, Inc. All Rights Reserved.