Open topic with navigation

TIBCO Rendezvous® 8.7.0

# Limitations

## Range Limitations

`rvtrace` cannot examine packets unless they traverse the immediate network segment in which `rvtrace` is running. For example, point-to-point conversations within or between other network segments are invisible to `rvtrace`. Most saliently, retransmission requests and retransmission rejections are point-to-point packets, so they are visible to `rvtrace` only when they either originate or terminate in the local network segment. Consequently, in some situations `rvtrace` can detect retransmission broadcasts, even though it cannot detect the point-to-point packets that request retransmissions.

Switched network environments (such as switched Ethernet, or ATM) further limit the usefulness of `rvtrace` as a diagnostic tool. Since switching hardware forwards every point-to-point packet directly to its destination host, `rvtrace` detects point-to-point packets only when they either originate or terminate in the computer running `rvtrace`. In some switched networks, you can ameliorate this situation by disabling switching behavior—for example, by setting one port to diagnostic mode, or by using a diagnostic utility. This tactic can yield the full stream of point-to-point packets in a limited portion of the network; run `rvtrace` in that portion.

In addition, some network switching hardware can route multicast packets to a network segment only when a host in the segment is actually listening to the corresponding multicast group. Such high specificity further limits the range of `rvtrace`.

## Interface Limitation

`rvtrace` supports only Ethernet interfaces.

`rvtrace` does not support these (or any other) non-Ethernet interfaces: Token Ring, FDDI, ATM.

## Platform Support and Limitations

`rvtrace` operates on all platforms that Rendezvous supports—except z/OS.

TIBCO supports `rvtrace` on Microsoft Windows platforms, but requires that you first obtain and install `WinPcap` (see Obtaining pcap).

Warning | However, we do not support `rvtrace` on Windows SMP (Symmetric Multi-Processor) platforms at this time. `WinPcap` does not support SMP platforms, and might not operate correctly in multiprocessor environments. For more information, see www.winpcap.org/misc/faq.htm.
Note | On Windows platforms, we strongly recommend that you upgrade to the most recent version of `WinPcap`.

Note | UnixWare places security restrictions on programs that open interfaces in promiscuous mode (such as `pcap`). To run `rvtrace` on UnixWare platforms, you must dedicate a separate physical interface for that purpose.

Note | Mac OS X does not support `rvtrace`.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2023. Cloud Software Group, Inc. All Rights Reserved.