Open topic with navigation

TIBCO Rendezvous® 8.7.0

# Remote Connection Information

These parameters specify the remote end of a neighbor connection.

## Remote Router Name

In most situations, a routing daemon identifies a neighbor using its unique router name (see Router Name).

(For a counterexample, see Seek Neighbor with Any Name.)

## Remote Host

Specify the location of a neighbor either as a resolvable hostname, or as the IP address of the computer in a remote network where the neighboring daemon is running.

## Remote Connect Port

The remote port is the TCP port number where the remote neighbor listens for a connection request from this routing daemon.

This parameter must match the local connect port of a routing table entry within the `rvrd` process on the neighboring host computer.

## Remote Public Certificate

When neighbors communicate using TLS, you must enter the public certificate of the authorized neighbor. For background information, see Certificates and Security on page 29 in TIBCO Rendezvous Concepts.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2023. Cloud Software Group, Inc. All Rights Reserved.