Open topic with navigation

TIBCO Rendezvous® 8.7.0

# Border Routing

For an introduction to the concepts of this feature, see Border Routing.

Tip | Border routing is an advanced feature. We recommend that you consult with TIBCO before deploying this feature.

Border routing restricts permissible configurations. When an `rvrd` process is configured as a border router, that border router must be the only routing table entry for the process.

As a result, you can configure an `rvrd` process either as a collection of one or more first-tier routers, or as exactly one border router. You cannot configure more than one border router in a process, nor mix first-tier and border routers in the same process.

To configure a process as a border router, type the new router name, and click the Add Border Router button.

You cannot remove a border router from an `rvrd` process.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2023. Cloud Software Group, Inc. All Rights Reserved.