Open topic with navigation

TIBCO Rendezvous® 8.7.0

# DateTime Format

The Rendezvous datatype TIBRVMSG_DATETIME indicates a value in DateTime format.

Rendezvous DateTime format encodes the time with microsecond accuracy. The total time range is approximately 17432 years on each side of the epoch (midnight, zero seconds into January 1, 1970).

In wire format, DateTime values are 8 bytes:

| • | 40 signed bits representing seconds (zero denotes the UNIX epoch, namely, 12:00am, January 1, 1970).

| • | 24 unsigned bits representing microseconds after the seconds value.

Although the program representations of DateTime values can be significantly larger than these 64 bits, the excess is unused at this time.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2023. Cloud Software Group, Inc. All Rights Reserved.