Open topic with navigation

TIBCO Rendezvous® 8.7.0

# Overlapping Subject Space

Consider two distinct distributed programs that use overlapping subject spaces—that is, they use some of the same subjects for their messages. When the two programs are deployed on the same physical network, each one receives messages from the other, which is inappropriate. To eliminate interference within the network, isolate each program to a separate UDP service.

Yet this solution within one network does not ordinarily keep the subject spaces separate when routing daemons connect two or more networks, because the routing daemon merges the subject spaces of its local networks.

Figure 61: Routing Daemons Merge Subject Spaces

For example, on the left side of Routing Daemons Merge Subject Spaces, the two UDP services `7500` and `7502` effectively separate one physical network (`K.foo.com`) into two disjoint subject spaces; that is, program `L2` cannot receive messages from program `S1`. Similarly, on the right side of Routing Daemons Merge Subject Spaces, two UDP services `7577` and `7588` effectively separate one physical network (`J.foo.com`) into two disjoint subject spaces. However, the routing daemons in this configuration merge the subject spaces of their local networks—effectively canceling the separation; that is, program `L2` does receive messages from program `S1`.

To restore the separation, configure an independent routing table entry for each local network, as in Independent Routing Table Entries Keep Subject Spaces Separate.

Figure 62: Independent Routing Table Entries Keep Subject Spaces Separate

In Independent Routing Table Entries Keep Subject Spaces Separate, each `rvrd` process contains two independent routers, which act as parts of two disjoint routes—keeping the data and subject spaces separate:

| • | Routing table entries `A` and `F` form a route connecting network `2` with network `3`.

| • | Routing table entries `B` and `G` form a route connecting network `1` with network `4`.

Notice that once again, program `L2` cannot receive messages from `S1`.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2023. Cloud Software Group, Inc. All Rights Reserved.