Open topic with navigation

TIBCO Rendezvous® 8.7.0

# Transport Scope

Rendezvous software distinguishes between two broad classes of transports, each with a different potential scope and a different delivery mechanism.

| • | A network transport delivers messages across a network, to processes on one or more hosts. It also can deliver messages to several processes on a single host.

All messages pass through a Rendezvous daemon process.

The service, network and daemon parameters of a network transport specify its scope within the network (see Network Transport Parameters).

| • | An intra-process transport delivers messages between program threads within a single process.

Intra-process messages do not pass through a Rendezvous daemon process; instead, they remain local within the program process. Intra-process messages are significantly faster than network messages.

Each program contains exactly one intra-process transport; the Rendezvous open call creates it automatically. Its scope is the program process. Any thread can dispatch intra-process events from an appropriate queue.

Programs can use intra-process messages to implement user events. For more information, see Intra-Process Transport and User Events.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2023. Cloud Software Group, Inc. All Rights Reserved.