Open topic with navigation

TIBCO Rendezvous® 8.7.0

# Redundant Routing Daemons for Fault Tolerance

Rendezvous routing daemons can cooperate for fault-tolerant service. Fault tolerance protects routing daemons against hardware failures, process failures and network segmentation.

In Fault Tolerance among Routing Daemons, two routing daemon processes, `E.Anet.moo.com` and `F.Anet.moo.com`, run on separate host computers, and serve the local client network `Anet.moo.com`; similarly, routing daemons `G.Bnet.moo.com` and `H.Bnet.moo.com` both serve local client network `Bnet.moo.com`. Neighbor links connect `E` with `G` and `H`, and also `F` with `G` and `H`. Although these neighbor links offer redundant paths from `Anet` to `Bnet`, the routing daemons cooperate to forward each message only once. In failure situations, the routing daemons automatically readjust to continue service smoothly.

The concepts of primary and secondary do not apply to redundant routing daemons. Instead load balancing parameters govern fault-tolerant behavior (see Load Balancing).

In groups of redundant routers (such as `E` and `F`), the router names must be distinct, the local network configurations must be identical, while the load balancing parameters along neighbor links may differ.

Notice that `E` and `F` are not neighbors, nor are `G` and `H`. It would be an error for neighbors to serve the same local network (see Common Topology Errors).

Figure 56: Fault Tolerance among Routing Daemons

Subtopics

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2023. Cloud Software Group, Inc. All Rights Reserved.