Open topic with navigation

TIBCO Rendezvous® 8.7.0

# VC.DISCONNECTED

Advisory

## Subject Name Syntax

    _RV.ERROR.SYSTEM.VC.DISCONNECTED
    _RV.INFO.SYSTEM.VC.DISCONNECTED

## Purpose

A virtual circuit connection has broken.

## Remarks

Virtual circuit transport objects (that is, both terminals of the circuit) present this advisory.

Error

The error advisory, `_RV.ERROR.SYSTEM.VC.DISCONNECTED`, indicates virtual circuit failure:

| • | Either terminal detects DATALOSS (that is, missing messages) on the circuit.

| • | Either terminal detects loss of the heartbeat signal from the opposite terminal.

Info

The informational advisory, `_RV.INFO.SYSTEM.VC.DISCONNECTED`, indicates graceful disconnection—that is, one of these cases:

| • | The process at the other end of the circuit exits.

| • | The process at the other end of the circuit explicitly destroys its virtual transport object.

| • | The process at this end of the circuit explicitly destroys its virtual transport object. (It presents this advisory before freeing its storage.)

## Message Fields

Field Name | Description
`description` | A string that describes the reason for the broken connection. This field has datatype `TIBRVMSG_STRING.`

## See Also

Virtual Circuits

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2023. Cloud Software Group, Inc. All Rights Reserved.