Open topic with navigation

TIBCO Rendezvous® 8.7.0

# C Datatypes

C Type | Type Description | Notes
`tibrv_``bool` | boolean | `TIBRV_``FALSE`, `TIBRV_``TRUE`
`tibrv_``f32` | 32-bit floating point |
`tibrv_``f64` | 64-bit floating point |
`tibrv_``i8` | 8-bit integer |
`tibrv_``i16` | 16-bit integer |
`tibrv_``i32` | 32-bit integer |
`tibrv_``i64` | 64-bit integer |
`tibrv_``u8` | 8-bit unsigned integer |
`tibrv_``u16` | 16-bit unsigned integer |
`tibrv_``u32` | 32-bit unsigned integer |
`tibrv_``u64` | 64-bit unsigned integer |
`tibrv_``ipaddr32` | 4-byte IP address | Stored in network byte order. String representation is four-part dot-delimited notation.
`tibrv_``ipport16` | 2-byte IP port | Stored in network byte order. String representation is a decimal integer (all 16-bits).
`tibrvMsg` `DateTime` | Rendezvous datetime struct | See tibrvMsgDateTime.
`tibrv_``f32*` | 32-bit floating point array |
`tibrv_``f64*` | 64-bit floating point array |
`tibrv_``i8*` | 8-bit integer array |
`tibrv_``i16*` | 16-bit integer array |
`tibrv_``i32*` | 32-bit integer array |
`tibrv_``i64*` | 64-bit integer array |
`tibrv_``u8*` | 8-bit unsigned integer array |
`tibrv_``u16*` | 16-bit unsigned integer array |
`tibrv_``u32*` | 32-bit unsigned integer array |
`tibrv_``u64*` | 64-bit unsigned integer array |
`tibrv` `Msg` | Rendezvous message | See tibrvMsg.
`char*` | character string | ISO 8859-1 (Latin-1) character encoding
`void*` | opaque byte sequence |

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2023. Cloud Software Group, Inc. All Rights Reserved.