Open topic with navigation

TIBCO Rendezvous® 8.8.0

# Beware of Network Boundaries

Rendezvous software can use a combination of multicast, broadcast and point‑to‑point network messages. If your network includes bridges and routers, some of these messages may not cross segment boundaries.

Sometimes the network equipment can be configured to pass and block exactly the right traffic. In other situations, you may need Rendezvous routing daemon to pass broadcast and multicast traffic across wide-area network boundaries. Consult your system administrator or network administrator.

## See Also

Routing Daemon (rvrd) in TIBCO Rendezvous Administration

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2025. Cloud Software Group, Inc. All Rights Reserved.