Open topic with navigation

TIBCO Rendezvous® 8.8.0

# Properties of Virtual Circuits

Properties

Virtual circuits guarantee these properties:

| • | All inbound messages come only from the opposite terminal. Senders outside of a virtual circuit cannot insert data into its message stream.

| • | All outbound messages go only to the opposite terminal. Listeners outside of a virtual circuit cannot receive its message stream.

| • | Terminals receive explicit feedback if the connection is interrupted. Programs can promptly detect failure of mission-critical components or communications, and act to restore or replace them.

Application Ideas

The first and second properties suggest virtual circuits for applications that must insulate its message streams against subject name interference.

The third property suggests virtual circuits for applications that require continuous communication, such as monitoring and control of manufacturing processes, no-loss data transmission, or data replication.

Migration Path

Rendezvous implements virtual circuit terminals as transport objects. When appropriate, you can easily convert most existing programs to use virtual circuits (instead of ordinary network transports) with only minor code changes.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2025. Cloud Software Group, Inc. All Rights Reserved.