Open topic with navigation

TIBCO Rendezvous® 8.8.0

# Data Capture Files

`rvtrace` can write packets into a capture file, and read a stream of packets from a file (as if from the network).

## Motivation

Packet capture files are an important tool for problem diagnosis. Several techniques are useful:

| • | Capture packet data for later analysis.

| • | Capture packet data for further analysis at a remote location.

| • | Capture packets at high speed, then replay later when I/O delays are acceptable.

In general, `rvtrace` can capture packets to a file faster than it can display statistics. Large amounts of display data can create I/O delays, which could cause `rvtrace` to miss packets. For example, in a heavily loaded network, displaying subject statistics for many subjects could have this undesirable result.

You can use data capture files to side-step this difficulty. For example, capture a five-minute snapshot of packets (capturing suppresses display); then replay packets from the file, displaying statistics when the consequences of I/O delays are no longer problematic.

## Output File Rotation

The rotation regimen for data capture output is almost identical to the rotation regiment for log files; see Log Rotation.

The only difference between them, is that `rvtrace` always deletes an older existing file before opening a file for writing packet data. (That is, it never appends to the end of an existing data capture file.)

## Output Rotation Backward Compatibility

| The command line option `-w-rotate` `total_size` is deprecated in release 7.5, and will become obsolete in a subsequent release. We recommend migrating to the new rotation parameters at your earliest convenience. In the meantime, we preserve backward compatibility by converting the value of this deprecated parameter to corresponding values of the new parameters:
| • | `-w-rotate` `total_size` retains its old meaning—specifying the total size for all data capture files. The maximum size for each individual file in the rotation is `total_size``/10`.
| • | If both old and new parameters are present, the new parameters take precedence (overriding the old parameter).

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2025. Cloud Software Group, Inc. All Rights Reserved.