Open topic with navigation

TIBCO Rendezvous® 8.8.0

# tibrvIOType

Type

## Declaration

    typedef enum {
       TIBRV_IO_READ,
       TIBRV_IO_WRITE,
       TIBRV_IO_EXCEPTION } tibrvIOType;

## Purpose

Distinguish event interest in I/O conditions.

Value | Description
`TIBRV_IO_READ` | The socket is now readable.
`TIBRV_IO_WRITE` | The socket is now write-available.
`TIBRV_IO_EXCEPTION` | An exceptional condition occurred on the socket. (For example, out-of-band data has arrived.)

## See Also

tibrvEvent_CreateIO()

tibrvEvent_GetIOType()

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2025. Cloud Software Group, Inc. All Rights Reserved.