Open topic with navigation

TIBCO Rendezvous® 8.8.0

# Control Message Sizes

Although the ability to exchange large data buffers is a feature of Rendezvous software, it is good practice to avoid sending messages that are too large. For example, to exchange data up to 10,000 bytes, a single message is efficient. But to send files that could be many megabytes in length, use multiple send calls, perhaps one for each record, block or track. Empirically determine the most efficient size for the prevailing network conditions. (The actual size limit is 64 MB, which is rarely an appropriate size.)

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2025. Cloud Software Group, Inc. All Rights Reserved.