Open topic with navigation

TIBCO Rendezvous® 8.8.0

# Principles of Operation

In our experience, Rendezvous distributed applications achieve optimal network performance when senders transmit messages in short batches, pausing briefly between batches. This observation is the foundation for the performance assessment tool.

Performance assessment software measures network performance by sending runs of messages, and compiling statistics. You can experiment by varying parameters such as message size, run length, batch size, pause interval—which affect the network data rate.

Each message contains s bytes of payload data (plus message headers and packet overhead).

`rvperfm` sends one or more sequences (or runs) of m messages to the network.

Instead of sending a continuous stream of messages, `rvperfm` groups them into batches of b messages, pausing for an interval of i seconds between the end of one batch and the start of the next batch.

While `rvperfm` is sending messages, zero or more process instances of `rvperfs` are listening for those messages and compiling statistics. At the end of each run, the `rvperfs` processes report back to `rvperfm`, which outputs the statistics.

Subtopics

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2025. Cloud Software Group, Inc. All Rights Reserved.