Open topic with navigation

TIBCO Rendezvous® 8.8.0

# Best Practice: Fault Tolerance in Second-Tier Networks

Border Router: Fault Tolerance illustrates fault tolerance in a second-tier network that crosses a WAN link. Notice that this topology addresses two aspects of fault-tolerance:

| • | Redundant border routers—BR1 and BR2

| • | Redundant routing across WAN communications—the X pattern spanning the first-tier routers L1, L2, M1 and M2 within zone B

Figure 84: Border Router: Fault Tolerance

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2025. Cloud Software Group, Inc. All Rights Reserved.