Open topic with navigation

TIBCO Rendezvous® 8.8.0

# Longest Service Interruption

In most situations, the longest service interruption is no longer than the activation interval.

## Cascading Failure Situations

Cascading failure is an unusual situation in which several members fail in succession—either as they activate, or toward the end of their activation interval. As a result, several activation intervals may elapse before service is restored (or the supply of inactive members is exhausted).

Cascading failure can result from fatal program errors during activation, or from a rare coincidence of unrelated failures.

## New Member Situations

When a new member joins a group, Rendezvous fault tolerance software identifies the new member to existing members (if any), and then waits for a period of one activation interval to receive identification from them in return. If, at the end of this interval, it determines that too few members are active, then it instructs the new member to activate.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2025. Cloud Software Group, Inc. All Rights Reserved.