Open topic with navigation

TIBCO Rendezvous® 8.8.0

# Services

On this page `rvd` displays information about the network services it mediates for its clients.

To display this page, click Services in the left margin of any page of the `rvd` browser administration interface.

Figure 49: rvd Services Page

Item | Description
table rows | Each row of the table describes one network service—that is, a UDP service on a particular network interface.
Service | The UDP service number. Clicking this number displays the Service Information page.
Network | The network number or multicast specification.
Hosts | The number of other host computers with Rendezvous daemons that communicate on this network and service.
Clients | The number of client transports that use this network and service.

## Service Information

Service

This page (see rvd Service Information Page) displays additional detail and operational statistics about a particular network service.

To display this page, click any service number in the Services page.

Figure 50: rvd Service Information Page

Item | Description
Service | The UDP service number.
Network | The network number or multicast specification.
Reliability | On this service, `rvd` retains outbound message data for retransmission. After this interval, it discards the data. For complete details, see Reliability and Message Retention Time.
Creation | Date and time that this service became active.
Clients | The number of client transports that use this network service. To view the Clients page, click this item.
Hosts | The number of other host computers with Rendezvous daemons that communicate on this network and service. To view the Host List page, click this item.
Subscriptions | The number of subscriptions registered with the daemon on this network service. To view the list of subscriptions, click this item.
Communication ID | Identifies the daemon and service. TIBCO support staff may request this value for diagnostic purposes.
Inbound Rates | The rate (per second) at which inbound messages, bytes and packets arrived on this network service during the most recent sampling period.
Outbound Rates | The rate (per second) at which the daemon sent outbound messages, bytes and packets on this network service during the most recent sampling period.
Inbound Counts | Cumulative statistics about inbound data messages; running totals since the start of the daemon process:
| • | msgs—number of messages
| • | bytes—number of bytes
Outbound Counts | Cumulative statistics about outbound data messages; running totals since the start of the daemon process:
| • | msgs—number of messages
| • | bytes—number of bytes
Inbound Packet Totals | Cumulative statistics about inbound packets; running totals since the start of the daemon process:
| • | pkts—number of data packets
| • | missed—number of missed packets (detected as a packet sequence gap)
| • | lost MC—number of multicast packets lost because the sending daemon could not retransmit them
| • | lost PTP—number of point-to-point packets lost because the sending daemon could not retransmit them
| • | suppressed MC—number of multicast packets for which the daemon suppressed the sending of retransmission requests (see Retransmission Control )
| • | bad pkts—number of unreadable data packets
These bad packets correspond to `DATALOSS` advisories in which the error description string includes the words`multicast destination`. For information about non-zero values see .
Outbound Packet Totals | Cumulative statistics about outbound packets; running totals since the start of the daemon process:
| • | pkts—number of data packets
| • | retrans—number of packets retransmitted (multicast and point-to-point)
| • | lost MC—number of multicast packets the daemon could not retransmit (too old)
| • | lost PTP—number of point-to-point packets the daemon could not retransmit (too old)
| • | shed MC—number of multicast packets for which the daemon ignored retransmission requests from a chronically-lossy receiver, and did not retransmit the data (see Retransmission Control )
| • | bad retreqs—number of unreadable retransmission request packets
These bad packets correspond to `DATALOSS` advisories in which the error description string includes the words`multicast destination`. For information about non-zero values see .
Information Alerts | This panel displays the 50 most recent `DATALOSS` advisories.

Subtopics

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2025. Cloud Software Group, Inc. All Rights Reserved.