Open topic with navigation

TIBCO Rendezvous® 8.8.0

# Heartbeats

Each active member of a fault tolerance group broadcasts a heartbeat signal to the other group members. The heartbeat signal is a regular, periodic stream of heartbeat messages. The heartbeat signal indicates that the member is still active.

When a process joins a fault tolerance group, it specifies its heartbeat interval as a parameter. This interval governs a repeating timer; each time the heartbeat interval elapses, Rendezvous fault tolerance software publishes a heartbeat message.

To determine the correct value for the heartbeat interval, see Step 4: Choose the Intervals.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2025. Cloud Software Group, Inc. All Rights Reserved.