Open topic with navigation

TIBCO Rendezvous® 8.8.0

# Network Parameter

Every network transport object communicates with other transport objects over a network. On computers with only one network interface, the Rendezvous daemon communicates on that network without further instruction from the program.

On computers with more than one network interface, the `network` parameter instructs the Rendezvous daemon to use a particular network for all communications involving this transport. To communicate over more than one network, a program must create a separate transport object for each network.

The network parameter also specifies multicast addressing details (for a brief introduction, see Multicast Addressing).

To connect to a remote daemon, the `network` parameter must refer to the network from the perspective of the remote computer that hosts the daemon process.

Subtopics

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2025. Cloud Software Group, Inc. All Rights Reserved.