Open topic with navigation

TIBCO Rendezvous® 8.8.0

# Activation Interval

Inactive members track the heartbeats of active members, detecting the loss of an active member when its heartbeat signal is silent for a duration called the activation interval. (The name activation interval refers to the use of this parameter as the time that an inactive member waits before becoming active when a heartbeat signal is lost.)

When a process joins a fault tolerance group, it specifies the activation interval as a parameter. All members of a group must specify the same activation interval. To determine the correct value, see Step 4: Choose the Intervals.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2025. Cloud Software Group, Inc. All Rights Reserved.