Open topic with navigation

TIBCO Rendezvous® 8.8.0

# Retransmission

Within its local networks, a routing daemon is the source (that is, the sending daemon) of all the forwarded messages that it rebroadcasts. That routing daemon handles retransmission requests (for example, if a listening application in the local network misses a packet).

Retransmission and rvrd illustrates this concept:

Procedure

| 1. | An application in network A sends a message.

| 2. | Routing daemon A forwards the message to routing daemon B.

| 3. | Routing daemon B rebroadcasts the message on network B.

| 4. | A receiving application in network B misses a packet, and its `rvd` requests retransmission.

| 5. | If the packet is within the reliability window of routing daemon B, then it retransmits the packet.

Otherwise, it denies the retransmission request; it does not attempt to get a new copy of the message from routing daemon A.

Figure 72: Retransmission and rvrd

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2025. Cloud Software Group, Inc. All Rights Reserved.