# Sample Output for XTUV,TRG Command

The following is an example of the output generated by the XTUV,TRG command:

## Field Descriptions for Output of XTUV,TRG

    XTUV TRG,NEXT 4

    CICS:C512WW3G, Location 2021B000, Size:15296
      Max Len:60000, Rep-TO:5000, XMC-TO:2, Mode:R
    Intf:REDEA1, Pri:1, Active, NoStress(0), NoThrottle(0), SSID:QA111RE1
      Pool 1  Max Size:1000      ThdCnt:0 URL:QA111RE1.REDEA1#P1.P1AMEA1
       Pacing:0 Retry:0 Lost:0 Sent:0 Error:0 Join:0
      Pool 2  Max Size:8192      ThdCnt:0 URL:QA111RE1.REDEA1#P2.P2AMEA1
       Pacing:0 Retry:0 Lost:0 Sent:0 Error:0 Join:0
    Intf:REDEA2, Pri:1, Active, NoStress(0), NoThrottle(0), SSID:QA111RE1
      Pool 1  Max Size:1000      ThdCnt:0 URL:QA111RE1.REDEA2#P1.P1AMEA2
       Pacing:0 Retry:0 Lost:0 Sent:0 Error:0 Join:0
      Pool 2  Max Size:8192      ThdCnt:0 URL:QA111RE1.REDEA2#P2.P2AMEA2
       Pacing:0 Retry:0 Lost:0 Sent:0 Error:0 Join:0
    Intf:REDEA3, Pri:1, Active, NoStress(0), NoThrottle(0), SSID:QA111RE1
      Pool 1  Max Size:1000      ThdCnt:0 URL:QA111RE1.REDEA3#P1.P1AMEA3
       Pacing:0 Retry:0 Lost:0 Sent:0 Error:0 Join:0
      Pool 2  Max Size:8192      ThdCnt:0 URL:QA111RE1.REDEA3#P2.P2AMEA3
       Pacing:0 Retry:0 Lost:0 Sent:0 Error:0 Join:0

     More... (Press Enter)

Field | Description
--- | ---
CICS | The current CICS region applid.
Location | Memory address of the RED CICS Trigger control block.
Size | The size of the memory area for the location mentioned.
Max Len | The value shows the AMSG-MAXLEN value that the RED interface uses as the maximum message length. If the application program attempts to send data of longer length through SXCOTRED, it fails.
Rep-TO | The wait time in milliseconds that the guaranteed Trigger process waits for the response from Substation ES.
XMC-TO | The maximum time in seconds that an XCF send trigger message operation is given to complete successfully.
Mode | R for Round-Robin; F for Primary-Alternate.
Intf | RED interface name, display up to total of eight RED interfaces.
Pri | The value shows that the parameter of AMSG-PRIORITY been set for the RED interface connection priority to the CICS region.
Active / InActive | Status of interface.
NoStress | The number of XCF interfaces that have been under stress condition.
NoThrottle | States whether we had a throttle and what the count of throttle has been.
SSID | Substation ES ID followed by Substation ES RED interface ID.
Pool | The related information of buffer pool #, where # can be 1, 2, or 3.
Max Size | The maximum message length that is allowed to be sent within a selected pool. If a message is larger than a specified value in the Max Size field but smaller or equal to the value in the field, RED handles the message differently, resulting in processing overhead.
ThdCnt | The number of concurrent message worker threads that the RED interface started to service trigger messages.
URL | The target member name that the RED interface uses to publish trigger messages.
Pacing | The number of microseconds that the RED interface trigger request waits after sending a trigger message from the buffer pool, before returning to the CICS application.
Retry | The number of times SXCOTRED attempts to resend a reliable and guaranteed trigger message if the first send fails.
Lost | The total number of reliable confirm and guaranteed trigger messages that have been resent after receiving a timeout error (with RED reason code 8110).
Sent | The total number of trigger messages that have been sent. This count includes any resend messages following a failure.
Error | The total number of trigger messages that were not sent because of an error.
Join | The total number of RED API JOIN calls that have been done.

Copyright © TIBCO Software Inc. All rights reserved.