# Execution Parameters of IVP Sender Listener

The following input control statement sets instruct the IVP Sender Listener to publish the corresponding request messages.

## Rendezvous – DPL Request/Reply (LANGUAGE C)

    SUBJ-REQ   tibss.CICS.C.Request
    RESOURCE   SXC3I001
    REPEAT     1
    TIMEOUT    15
    WAIT       0
    BES-DELAY  5

## Rendezvous – DPL MRO Request/Reply (LANGUAGE C)

    SUBJ-REQ   tibss.CICS.MRO.Request
    RESOURCE   SXC3I001
    REPEAT     1
    TIMEOUT    15
    WAIT       0
    BES-DELAY  5

## Enterprise Message Service – DPL Request/Reply (LANGUAGE C)

    DEST-REQ   tibss.CICS.C.Request
    DEST-REP   tibss.CICS.C.Reply
    TYPE       QUEUE
    RESOURCE   SXC3I001
    REPEAT     1
    TIMEOUT    15
    WAIT       0
    BES-DELAY  5

## Enterprise Message Service – DPL Request/Reply (LANGUAGE COBOL)

    DEST-REQ   tibss.CICS.Cobol.Request
    DEST-REP   tibss.CICS.Cobol.Reply
    TYPE       QUEUE
    RESOURCE   SXCCI001

## Enterprise Message Service – DPL MRO Request/Reply (LANGUAGE COBOL)

    DEST-REQ   tibss.CICS.MRO.Request
    DEST-REP   tibss.CICS.MRO.Reply
    TYPE       QUEUE
    RESOURCE   SXCCI001

Copyright © TIBCO Software Inc. All rights reserved.