# Buffer Definitions Panel

You can define or modify a buffer definition in the Buffer Definitions panel.

## Panel Layout

    SXTP02 ----------------------- Buffer Definitions ------------ Row 1 to 1 of 1
    Command ===>                                                   Scroll ==> CSR

     (ADD=Create new Buffer, CAN=Cancel updates, F=Find)
    Sel Flds Buffer Id
    -   ---- ----------------
           0 New-Buffer1
    ******************************* Bottom of data ********************************

## Field Description

The following table lists the fields in the Buffer Definitions panel:

Field | Description
--- | ---
Command | You can enter `ADD` to create a new buffer definition, and enter `CAN` to cancel all modifications just done to the existing buffer definition. Enter F xyz to bring the xyz buffer definition to the top of the list. Valid commands: ADD, CAN and F.
Sel | You can select an existing buffer definition to modify. Valid selections: S(elect), D(elete), R(epro), and U(sedon). If you select U, you can access the panel described in Conversion Rules using Buffer Definition Panel.
Flds | The total number of fields in the buffer definition.
Buffer Id | Required. The user defined name of the buffer definition. Default value: New-Buffer1.

Copyright © TIBCO Software Inc. All rights reserved.