# IVP IMS Conversational Sender or Listener

The program `SXR3ICV1` works as a TIBCO messaging transactional client application. The Conversational Sender or Listener publishes Substation ES IMS Conversational IVPs requesting messages. Which messages are requested depends on a set of parameters passed in through `SYSIN` DD statements in the run JCL.

Each output resulting from the IMS application is written to the log output medium. The sample JCL stream is in the following:

Data Set: `USERHLQ.JCL`

Member: `SXIRICVS`

Note: The `EXEC PARM - IVPNETW` is substituted with a set of TIBCO Rendezvous transport parameters. It is recommended that you use the provided default settings for all IVP runs. To use the other settings, see the TIBCO Rendezvous Administration manual for information on the parameters.
Copyright © TIBCO Software Inc. All rights reserved.