# Administration Messages

The following table describes the administration messages.

Code | Description
--- | ---
`SXA1008I` | Substation ID:SS-Id VVersion
Explanation: Displays the Substation ES Identifier and the version number. Destination: `TIBLOG` and/or Remote Request Response.
`SXA2600I` | TIB/SS Console Interface - Awaiting Command Request
Explanation: This message is displayed on the z/OS console when the Write to Operator console interface type is selected in the Substation ES Initialization Parameter. Operations personnel respond to the outstanding request when commands must be issued for the Substation ES to process. Destination: z/OS console.
`SXA2601I` | Console Command 'keyword value'
Explanation: This message echoes an operator-entered Substation ES console command.
`SXA2602I` | Remote Command 'keyword value'
Explanation: This message echoes an operator command sent from a remote application or the Substation ES General Utility.
`SXA2603E` | Invalid Value: Value supplied for Keyword: Keyword
Explanation: An invalid Value has been specified for a valid Keyword command. User Response: Supply the correct values and reissue the command.
`SXA2604W` | No HELP available for Keyword: Keyword
Explanation: No help is available for Keyword.
`SXA2605E` | Invalid Value: Value supplied for Command: Command
Explanation: An invalid value (Value) has been supplied for Command. User Response: Specify the correct value and reissue the operator command. See the TIBCO Substation ES Installation manual for the console commands.
`SXA2606E` | Incomplete specification for Command: value
Explanation: An operator command received by Substation ES is only partially complete. Not all the necessary keywords or values needed to process the command have been supplied. User Response: See the TIBCO Substation ES Installation manual for the correct command syntax. Correct and resubmit the command.
`SXA2607I` | Received Remote command text, Scheduled for processing
Explanation: The remote command text has been received and is scheduled for processing. No additional reply information will be sent to the user because this type of command is scheduled internally and will be processed at some appropriate point.
`SXA2607W` | Command may only be entered via console text
Explanation: The remote command text can only be submitted on the host system by an authorized operator. User Response: Contact your Substation ES support representative about authorization.
`SXA2608E` | Unsupported Value:value supplied for CEMT Command
Explanation: Substation ES only supports CEMT inquire commands. User Response: Enter CEMT `I/INQ/INQUIRE` with optional sub-commands to execute the request successfully.
`SXA2609I` | Operator issued <STOP> command via console
Explanation: An operator has issued a z/OS stop command from a console. System Action: Substation ES is shut down normally. Destination: `TIBLOGPR.`
`SXA2610E` | Invalid Keyword supplied keyword
Explanation: An invalid console keyword command has been supplied. User Response: See the TIBCO Substation ES Operations and Administration manual for the console commands.
`SXA2610I` | Available Console Command Keywords:
Explanation: When the `HELP` console keyword is issued, this header message precedes message `SXG2613I`, which lists the valid console keywords.
`SXA2611E` | Invalid Keyword: keyword supplied for command: command
Explanation: An invalid keyword has been supplied for this console command. User Response: See the TIBCO Substation ES Operations and Administration manual for the console commands and keywords.
`SXA2613I` | Text
Explanation: This is a general console reply. Console-command replies are formatted with this message ID, which displays the output.
`SXA2614I` | Run-Time value keyword changing from old-value to new-value
Explanation: A Substation ES console or operator command has been issued, requesting that the operational parameter keyword be reset or changed. The current value is shown as old-value and the required value is shown as new-value. System Action: Substation ES updates the operational runtime setting to new-value.
`SXA2615E` | Interface ID required for command:Cmd
Explanation: An interface ID was required for this command and was not specified on the request submitted. Destination: `TIBLOG` and/or Remote Request Response.
`SXA2616I` | IId:Intf-Id Trigger `TRCLVL` changing from old-value to new-value
Explanation: A Substation ES operational command has been issued, requesting that a trigger trace level be changed. The current value is shown as old-value and the supplied value is shown as new-value. System Action: Substation ES updates the operational runtime setting to new-value.
`SXA2617E` | IId:Intf-Id Interface specified is invalid for request
Explanation: The Interface specified for the issued operational command is invalid. The Substation ES interface is either not able to process the command specified, or is not eligible to execute the command. System Action: Specify the correct interface identifier.
`SXA2619E` | Keyword Value not found
Explanation: The keyword specified shown is required and could not be found in the command entered. System Action: Specify the correct operational command and reissue the operator command. See the TIBCO Substation ES Operations and Administration manual for the console commands.
`SXA2620I` | Operational Request successfully processed
Explanation: This message indicates that an operational command has completed its scheduled execution.
`SXA2621I` | IId:Intf-Id, Operational Request successfully processed
Explanation: A command sent to another interface to process has successfully executed.
`SXA2623E` | Missing Keyword: Name in Command: command
Explanation: A keyword (Name) was expected to be present in an operational command (command), but has not been specified. User Response: Supply the correct command and keyword with values required and reissue the command.
`SXA2626E` | Console call failed. RC:RC Reason: Rsn
Explanation: A call to the z/OS console routine SXGAF024 failed. User Response: Contact TIBCO Support with the information on the error from the log and trace files.
`SXA2629E` | Invalid length (number) for value:command issued
Explanation: A operational command was issued but the length of the command most likely exceeds the allowable length which is 120 characters. User Response: Review the command to ensure the correct value is specified. If the problem persists, contact TIBCO Support with the information on the error from the log and trace files. System Action: The request fails.
`SXA2631I` | Console Commands only written to the Log
Explanation: An echo of the console commands with the resulting output is only recorded to the log file’s destination. User Response: None. You can echo console commands and results on the z/OS master terminal by specifying the appropriate value for the `CONSOLE-MSG` System Initialization Parameter keyword.
`SXA2632I` | This command has no reply: command
Explanation: The Substation ES operational command command has been issued but there will be no reply from its operation. System Action: Substation ES updates the operational runtime settings.
`SXA2633I` | Nothing (more) to display
Explanation: There is nothing more to display.
`SXA2640I` | Starting ~ HeartBeats
Explanation: The Substation ES HeartBeat function has been requested by the user and is now starting to send events to the requested trigger service. The content of the specified operational command(s) is sent to the desired destination. System Action: Substation ES sends interval heartbeat updates until the connection it sends its delivery on is stopped or a shutdown is performed. If the connection is reestablished the heartbeat will continue again.
`SXA2641I` | Terminating ~ HeartBeats
Explanation: The Substation ES HeartBeat function has been stopped. System Action: Substation ES stops sending the heartbeats at the specified interval until the reason for its termination has been resolved.
`SXA2690E` | Operations Request has been unsuccessful
Explanation: An operator command received from a remote application did not execute successfully. User Response: Review any additional warnings, error messages, and reason codes in the log file to determine the cause for the error condition. If you cannot resolve the error, contact TIBCO Support with the log and trace files.
`SXA2645I` | HeartBeat sent its information
Explanation: When the trace level is set at 4 or higher, this message denotes that the trace request has been executed and the information will now be sent to the service for delivery. User Response: None.
`SXA2645E` | HeartBeat Stopped. Description
Explanation: HeartBeat stopped after having recorded 10 errors for this activity. User Response: Review previous messages in the Log file that might indicate the reasons for this message.
`SXA2691E` | Operational functions disabled due to errors
Explanation: Failure to allocate the storage for operations results in this facility being disabled. User Response: Contact TIBCO Support and report the issue supplying the log, trace, and audit files. System Action: Processing continues without administration and operational capabilities.
`SXA2693E` | Operational request unsuccessful - Notification
Explanation: Substation ES operations has received a notification from another asynchronous process that it failed at some point during its execution. It also posts this notification to remote processes. User Response: Review the preceding messages in the Substation ES log to determine the possible cause of the error. If you cannot resolve the error, contact TIBCO Support with the information on the error from the log and trace files. System Action: Substation ES continues to execute normally without disruptions.
`SXA2650I` | Internal Command value
Explanation: A Substation ES internal administrative command shown in value has been requested. If any actions are taken by Substation ES, the messages are shown in the Log file following this command. User Response: None.
`SXA2666I` | End-of-Command
Explanation: This is the end of a console reply.
`SXA2675I` | Requesting Auto Recovery for BES: Intf-Id
Explanation: Substation ES issues this message when auto recovery is in progress for an interface. If this value applies to all interfaces, then an asterisk (*) is displayed. User Response: None. System Action: After a reconnect to an IMS or CICS system is completed, Substation ES schedules an auto recover command to ensure that all services using this interface and that have a service level of guaranteed will obtain their messages from the EMS queues, and process them.
`SXA2676I` | Requesting Auto Recovery for RID:RID=R-Name
Explanation: Substation ES issues this message when auto recovery is in progress for a Recipe Service. User Response: None. System Action: A user has requested an explicit RECOVER for a particular Recipe Service to obtain messages that might possibly be located in the EMS queue and process them.
`SXA2685I` | Suspending all services for BES:Intf-Id
Explanation: This is a follow-up message that is issued after the message `SXA2650I`. It indicates that all services for this BES will be suspended because of the internal command issued. User Response: None.
`SXA2694E` | IPC Unknown Reply event received: num
Explanation: Substation ES Internal Process Communications has received an invalid event and does not know how to handle this reply. User Response: Contact TIBCO Support with the information on the error from the log and trace files. System Action: Substation ES continues to execute normally without disruptions.
`SXA2695E` | Write to Operator failure, RC: RC
Explanation: An operator command received by the Substation ES administration subtask has failed to execute. User Response: Review any additional warning or error messages and reason codes in the log file to determine the cause for the error. Contact TIBCO Support with the information on the error from the log and trace files.

Copyright © TIBCO Software Inc. All rights reserved.