# Request or Reply

To demonstrate request or reply message processing, the Substation ES IVP Sender Listener publishes a message (using a selected messaging application) to Substation ES. Substation ES receives the message, transforms the data contents, and forwards the information to the appropriate BES.

Upon completion, an acknowledgment or result set is returned to the Substation ES IVP Sender Listener through Substation ES.

Copyright © TIBCO Software Inc. All rights reserved.