# Command Summary

The following table summarizes all Substation ES console commands by category. If multiple keywords are enclosed within square brackets, you must specify one of those keywords with the command.

## Display

Command | Keyword
--- | ---
HELP | [,sub-command]
SHOW, | ACTIVE|ACT,LISTENERS|LSNS[,INTF|IID=intf-id]
ACTIVE|ACT,RECIPE|RID[,INTF|IID=intf-id]
ACTIVE|ACT,TRIGGER|TID[,INTF|IID=intf-id]
SHOW, | CICS,“CEMT Sub-command”[,INTF|IID=intf-id]
CICS,SXTH[,Sub-command][,INTF|IID=intf-id]
SHOW, | DISABLED|DISA[,INTF|IID=intf-id]
DISABLED|DISA,LISTENERS|LSNS[,INTF|IID=intf-id]
DISABLED|DISA,RECIPE|RID[,INTF|IID=intf-id]
DISABLED|DISA,TRIGGER|TID[,INTF|IID=intf-id]
SHOW, | EMS,STATS,RECIPE|RID=name[,INTF|IID=intf-id]
SHOW, | ESB|TPORT[,INTF|IID=intf-id]
SHOW, | IMS,BUFFER
IMS,STATS
IMS,CONNECT
IMS,XCF
SHOW, | INTF|IID
INTF|IID=name
INTF|IID[,CONNECT|CONN]
INTF|IID=name[,CONNECT|CONN]
SHOW, | LOGSTATS
LOGSTATS,ALL
LOGSTATS,DETAIL
SHOW, | LTAVERS
SHOW, | QUE
QUE,LOCK
SHOW, | RED,BUFFER
RED,LIMIT
RED,SENDER=*|XCF sender name
RED,"CEMT Sub-commands"[,INTF|IID=intf-id]
RED,"XTUV[,Sub-commands"][,INTF|IID=intf-id]
SHOW, | RECIPE|RID|TRIGGER|TID=name,INTF|IID=intf-id
SHOW, | RV,DISPQ
RV,DQ-DISPQ
SHOW, | SSHOT[,num]
SSHOT,DETAIL|DET[,num]
SSHOT,ENTRY|ENT[,num]
SHOW, | SSID
SHOW, | SUSPENDED
SHOW, | SYS[,DEBUG]
SYS,LOCK
SHOW, | TRCSTATS
TRCSTATS,ALL
TRCSTATS,DETAIL
SHOW, | UOW
SHOW, | XCF,GRP[=Group name][,Member name]

## Update

Command | Keyword
--- | ---
DISABLE, | RECIPE|RID=name[,FOR=BES-Name,INTF|IID=intf-id]
RECIPE|RID=*,FOR=BES-Name[,INTF|IID=intf-id]
TRIGGER|TID=name[,INTF|IID=intf-id]
ENABLE, | RECIPE|RID=name[,FOR=BES-Name,INTF|IID=intf-id]
RECIPE|RID=*,FOR=BES-Name[,INTF|IID=intf-id]
SUSPENDED [,FOR=BES-Name, INTF|IID=intf-id]
TRIGGER|TID=name[,INTF|IID=intf-id]
RECOVER, | RECIPE|RID=name[,INTF|IID=intf-id]/*[,INTF|IID=intf-id]/*[,FOR=BES-Name,INTF|IID=intf-id]
REFRESH|REFR, | RECIPE|RID=name[,INTF|IID=intf-id][,TRCLVL=value]
TRIGGER|TID=name[,INTF|IID=intf-id][,TRCLVL=value]
COUNTERS
RECIPE|RID|TRIGGER|TID,ALL[,INTF|IID=intf-id]
TPORT=tport-id[,INTF|IID=intf-id]
RELOAD, | RECIPE|RID=name[,INTF|IID=intf-id]
TRIGGER|TID=name[,INTF|IID=intf-id]
RECIPE|RID|TRIGGER|TID,ALL[,INTF|IID=intf-id]
SUSPEND, | *,FOR=BES-Name[,INTF|IID=intf-id]

## Initialization

Command | Keyword
--- | ---
CONNECT|CONN, | INTF|IID=intf-id
APPLID=applid
ESB|TPORT=tport-id,INTF|IID=intf-id
DISCONNECT|DISCONN, | INTF|IID=intf-id
APPLID=applid
ESB|TPORT=tport-id,INTF|IID=intf-id
UNLOAD|UNL, | RECIPE|RID=name[,INTF|IID=intf-id]
TRIGGER|TID=name[,INTF|IID=intf-id]

## Control

Command | Keyword
--- | ---
SET, | CICS,STATS={Y|N}[,INTF|IID=intf-id]
SET, | CICS,TRCLVL-ONL=value[,INTF|IID=intf-id]
SET, | CICS,TRCLVL-HVS=value[,INTF|IID=intf-id]
SET, | CICS|IMS,TRCLVL-TRIG=value[,INTF|IID=intf-id]
SET, | IMS,BUFFER-PURGE[,INTF|IID=intf-id]
SET, | IMS,FREE-TRIG[,INTF|IID=intf-id]
SET, | IMS,HOLD-TRIG[,INTF|IID=intf-id]
SET, | IMS,REL-TRNAK[,SXITRNAK|DFS$$TOQ]
SET, | LOGDEST=value
SET, | LOGLVL=value
SET, | LOGFWRITE=value
SET, | RED,ABEND-RESET[,INTF|IID=intf-id]
SET, | RED,TRCLVL-AMSG|TRCLVL-SSRED|TRCLVL-CICS|TRCLVL-#RED|TRCLVL-TRG|TRCLVL-VIEW=value
SET, | RED,STATS|STATISTICS={Y|N},INTF|IID=intf-id]
SET, | RVFT[=value],INTF|IID=intf-id
SET, | STATS={Y|N}
SET, | STATS={Y|N}[,INTF|IID=intf-id]
SET, | TRACE-ENTRY=CONFIG,DETAIL
SET, | TRCDEST=value
SET, | TRCLVL=value[,OTMA|OPS|RR]
SET, | TRCFWRITE=value
SHUT
SWITCH
TERM

Copyright © TIBCO Software Inc. All rights reserved.