# Sample Output for XTUV,STATS Command

The following is an example of the output generated by the XTUV,STATS command:

    XTUV STATS

    LPAR:LION Job:CICSPRO  Member:TIBSS.MSGS#YODA
    XCF Status     :Active    RED Status     :Active    Buffer OvrFlow :0
    Msgs Discarded :0         Msgs Expired   :0         Msgs Held      :0

    Buffer Size    :8460      Msgs > Buff Sz :0
    Msgs Received  :156       Largest Size(R):1020      Max Msg Occ    :0
    Msgs in Pool   :0         Buf Size Ovr   :0         HWM Buffers    :1
    Msg Reply      :78        Msg Reply(SNC) :0         Msg SNC NAck   :0
    Req/Reply      :0         Req/Reply Fail :0         Msg RC4        :0
    SNC Sig(S)     :78        SNC Sig(R)     :0
    Mux Executes   :156       Mux Abend      :0         Mux Msg Lost   :0

Field Descriptions for output of XTUV,STATS

Field | Description
--- | ---
LPAR | The name of the Mainframe HUB being used for this URL registration.
Job | Name of the job creating the RED URL member.
Member | RED url target node.
XCF Status | How XCF sees this entry.
RED Status | How RED sees this entry.
Buffer OvrFlow | Number of times a message arrived and triggered the throttle event.
Msgs Discarded | Number of messages that were thrown away for error situations.
Msgs Expired | Number of messages that were removed from the buffer pool due to a timestamp expiration
Msgs Held | Number of messages with locks in the buffer pool.
Buffer Size | Size of each buffer set on the "JOIN".
Msgs > Buff Sz | Number of messages received that were greater than buffer size but less than Max size.
Msgs Received | Number of messages received for this buffer pool url.
Largest Size(R) | Size of largest message received.
Max Msg Occ | Number of times max Msg size received.
Msgs in Pool | Number of messages in the buffer pool (whether given to a receive api or not).
Buf Size Ovr | Number of messages received that were over buffer size.
HWM Buffers | High water Mark of messages in the buffer pool.
Msg Reply | Number of messages received that were replies to a SEND-R api.
Msg Reply(SNC) | Number of messages received that were confirmation events to a SEND-C.
Msg SNC NAck | Number of messages received that were non-confirmation events to a SEND-C.
Req/Reply | Number of messages sent (Req/Reply).
Req/Reply Fail | Number of R/R Msgs not getting reply.
Msg RC4 | Number of times XCF returned a return code of 4.
SNC Sig(S) | SNC confirmation signals sent.
SNC Sig(R) | SNC confirmation siganls received.
Mux Executes | Message User EXIT execution count.
Mux Abend | Message User EXIT Abend count.
Mux Msg Lost | Message User EXIT Abend Lost Msgs.

Copyright © TIBCO Software Inc. All rights reserved.