# Substation ES Console Interface

You can enter Substation ES operational commands through Substation ES Console Interface or remotely from applications. Commands that are received and the resultant output are logged to the Substation ES log medium.

If commands must be echoed upon the master console, you can set an appropriate value for the `CONSOLE-MSG` keyword in the Substation ES `SXSSIP$1` member.

Remote applications can issue all commands, except for the following ones:

- Commands to terminate Substation ES
- Commands to start or stop any of the Substation ES interfaces

From a remote location, you can send commands from a user application or Generic Listener or Sender Utility in Substation ES.

Copyright © TIBCO Software Inc. All rights reserved.