# Transferring the Initial Installation File

To transfer the Substation ES initial installation file from a LAN server or PC to the z/OS host, you can use JCL that contains the statements required for the file transfer.

The following sample JCL uses FTP to copy the Substation ES initial installation file from a LAN server or PC to the z/OS host.

    //#JOBNAME JOB (&SYSUID),'SUBSTATION ES FTP',CLASS=A
    //*
    // SET FTPADDR=10.10.2.99 < IP Address or Host Name
    //*
    //FTP EXEC PGM=FTP,REGION=0M,PARM='&FTPADDR (TIMEOUT 20'
    //SYSPRINT DD SYSOUT=*
    //OUTPUT DD SYSOUT=*
    //SYSTCPD DD DISP=SHR,DSN=TCPIP.PROFILE(FTPDATA) < Host Member
    //INPUT DD *
    lan-userid
    lan-password
    cd /lan-file-dir
    binary
    LOCSITE RECFM=FB LRECL=80 BLKSIZE=27920 CYL PRI=2 SEC=1
    get srvhlq.sxs.xmit.inst 'USERHLQ.XMIT.INST'(REPLACE
    quit
    /*
    //

Copyright © TIBCO Software Inc. All rights reserved.