# Metadata Configuration

Metadata configuration refers to the configuration items (recipes and triggers) that perform data exchanges between TIBCO applications and the transaction processing applications on z/OS.

The configuration items are entered and updated in the ESB Interface configuration panels. Those items that describe TIBCO messages and transaction input are located within a VSAM LDS file. Substation ES has a number of features for managing the flow and exchange of data between applications.

Copyright © TIBCO Software Inc. All rights reserved.