# Transformer User Messages

The following table describes the Transformer user messages.

Code | Description
--- | ---
`SXT5101E` | RV-Type is undefined
Explanation: The Rendezvous Type field is not on the list of fields that can be processed. User Response: Correct the recipe definition. System Action: The Input field is not processed.
`SXT5102E` | RV-ARRAYs are not supported
Explanation: The Rendezvous array types are not supported. User Response: Correct the recipe definition. System Action: The Input field is not processed.
`SXT5103E` | RV-User types are not supported
Explanation: Rendezvous user types are not supported. User Response: Correct the recipe definition. System Action: The Input field is not processed.
`SXT5104E` | Receiving field too short
Explanation: The receiving field is too short for the input data. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5105E` | Receiving field too long
Explanation: The incoming data field is greater than 8 bytes which is the maximum for a binary number. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5106E` | Receiving field has invalid length
Explanation: The receiving field has an invalid length. User Response: Correct the recipe definition. System Action: The Input field is not processed.
`SXT5107E` | Numeric overflow
Explanation: The receiving numeric field is too small for the input data. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5108E` | String or Text overflow
Explanation: The receiving string or text field is too small for the input data. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5109E` | Input value is not numeric
Explanation: The input value is not numeric. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5110E` | Input float value invalid
Explanation: The value of a float field is invalid. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5111E` | Date-Time conversion error
Explanation: An error occurred during the conversion to or from a date-time value. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5112E` | U64 with high-order bit on
Explanation: U64 with high-order bit is on. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5113E` | Decimal adjust error
Explanation: An error occurred during the adjustment of the placement of the decimal point. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5114E` | Input string too large to pack
Explanation: An input string is too large to pack into a packed decimal field. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5115E` | Packed operation too large
Explanation: A packed value contains too many significant digits. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5116E` | Unknown buffer field type
Explanation: The buffer definition contains an unknown type field. User Response: Correct the recipe definition. System Action: The Input field is not processed.
`SXT5117E` | Input RV-MSG not supported
Explanation: `RV-MSG` is not supported at the field level. User Response: Correct the definition or input data. System Action: The Input field is not processed.
`SXT5118E` | Input ENCRYPT not supported
Explanation: The Rendezvous type `ENCRYPT` is not supported. User Response: Correct the definition or input data. System Action: The Input field is not processed.
`SXT5119E` | Input NONE not supported
Explanation: The Rendezvous type `NONE` is not supported. User Response: Correct the definition or input data. System Action: The Input field is not processed.
`SXT5120E` | Input XML not supported
Explanation: The Rendezvous type XML is not supported. User Response: Correct the definition or input data. System Action: The Input field is not processed.
`SXT5121E` | Cannot convert OPAQUE to PACKED
Explanation: Conversion of `OPAQUE` to `PACKED` has failed. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5122E` | Cannot convert OPAQUE to ZONED DECIMAL
Explanation: Conversion of `OPAQUE` to `ZONED DECIMAL` has failed. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5123E` | Cannot convert OPAQUE to UNSIGNED BINARY
Explanation: Conversion of `OPAQUE` to `UNSIGNED BINARY` has failed. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5124E` | Cannot convert OPAQUE to BINARY
Explanation: Conversion of `OPAQUE` to `BINARY` has failed. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5125E` | Cannot convert OPAQUE to FLOATING POINT
Explanation: Conversion of `OPAQUE` to `FLOATING POINT` has failed. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5126E` | Cannot convert IPADDR32 to PACK
Explanation: Conversion of `IPADDR32` to `PACK` has failed. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5127E` | Cannot convert IPADDR32 to ZDEC
Explanation: Conversion of `IPADDR32` to `ZDEC` has failed. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5128E` | Cannot convert IPADDR32 to FLOAT
Explanation: Conversion of `IPADDR32` to `FLOAT` has failed. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5129E` | Cannot convert OPAQUE to U-PACKED
Explanation: Conversion from `OPAQUE` to Unsigned packed is not supported. User Response: Correct the conversion rule or input message. System Action: The conversion is marked as error.
`SXT5130E` | Cannot convert OPAQUE to UZ-DEC
Explanation: Conversion from `OPAQUE` to Unsigned zoned decimal is not supported. User Response: Correct the conversion rule or input message. System Action: The conversion is marked as error.
`SXT5131E` | Cannot convert IPADDR32 to UPACK
Explanation: Conversion from `IPADDR32` to Unsigned packed is not supported. User Response: Correct the conversion rule or input message. System Action: The conversion is marked as error.
`SXT5132E` | Cannot convert IPADDR32 to UZDEC
Explanation: Conversion from `IPADDR32` to Unsigned zoned decimal is not supported. User Response: Correct the conversion rule or input message. System Action: The conversion is marked as error.
`SXT5201E` | RV-Type is undefined
Explanation: The Rendezvous Type field is not on the list of fields that can be processed. User Response: Correct the recipe definition. System Action: The Input field is not processed.
`SXT5202E` | RV-ARRAYs are not supported
Explanation: The Rendezvous array types are not supported. User Response: Correct the recipe definition. System Action: The Input field is not processed.
`SXT5203E` | RV-User types are not supported
Explanation: The Rendezvous user types are not supported. User Response: Correct the recipe definition. System Action: The Input field is not processed.
`SXT5205E` | Receiving field has invalid length
Explanation: The receiving field has an invalid length User Response: Correct recipe definition. System Action: The Input field is not processed.
`SXT5206E` | Numeric overflow
Explanation: The receiving numeric field is too small for the input data. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5207E` | Input value is not numeric
Explanation: The input value is not numeric. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5208E` | Input float value invalid
Explanation: The value of a float field is invalid. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5209E` | Decimal adjust error
Explanation: An error occurred during the adjustment of the placement of the decimal point. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5210E` | Input string too large to pack
Explanation: An input string is too large to pack into a packed decimal field. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5211E` | Sending field too long
Explanation: The sending field is too long. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5212E` | Sending length is not positive
Explanation: The sending field is described by a nonpositive length. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5213E` | IPADDR32 string is invalid
Explanation: The sending field is not in the proper IPADDR32 format. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5214E` | Unknown buffer field type
Explanation: The buffer definition contains an unknown type field. User Response: Correct the recipe definition. System Action: The Input field is not processed.
`SXT5215E` | Output RV-MSG not supported
Explanation: `RV-MSG` is not supported at the field level. User Response: Correct the recipe definition or input data. System Action: The Input field is not processed.
`SXT5216E` | Output ENCRYPT not supported
Explanation: The Rendezvous type ENCRYPT is not supported. User Response: Correct the recipe definition. System Action: The Input field is not processed.
`SXT5217E` | Output NONE not supported
Explanation: The Rendezvous type NONE is not supported. User Response: Correct the recipe definition. System Action: The Input field is not processed.
`SXT5218E` | Output XML not supported
Explanation: The Rendezvous type `XML` is not supported. User Response: Correct the recipe definition. System Action: The Input field is not processed.
`SXT5219E` | Cannot convert [STRING | TEXT] to DATETIME
Explanation: Conversion of `STRING` or `TEXT` to `DATETIME` failed. User Response: Correct the recipe definition. System Action: The Input field is not processed.
`SXT5220E` | Cannot convert PACK to IPADDR32
Explanation: Conversion of `PACK` to `IPADDR32` has failed. User Response: Correct the recipe definition. System Action: The Input field is not processed.
`SXT5221E` | Cannot convert ZDEC to IPADDR32
Explanation: Conversion of `ZDEC` to `IPADDR32` has failed. User Response: Correct the recipe definition. System Action: The Input field is not processed.
`SXT5222E` | Cannot convert FLOAT to IPADDR32
Explanation: Conversion of `FLOAT` to `IPADDR32` has failed. User Response: Correct the recipe definition. System Action: The Input field is not processed.
`SXT5223E` | Cannot convert OPAQUE to DATETIME
Explanation: Conversion of `OPAQUE` to `DATETIME` has failed. User Response: Correct the recipe definition. System Action: The Input field is not processed.
`SXT5224E` | Cannot convert OPAQUE to binaries
Explanation: Conversion of `OPAQUE` to binary fields has failed. User Response: Correct the recipe definition. System Action: The Input field is not processed.
`SXT5225E` | Cannot convert OPAQUE to any float
Explanation: Conversion of `OPAQUE` to floating point fields has failed. User Response: Correct the recipe definition. System Action: The Input field is not processed.
`SXT5226E` | Cannot convert OPAQUE to BOOL
Explanation: Conversion of `OPAQUE` to `BOOL` has failed. User Response: Correct the recipe definition. System Action: The Input field is not processed.
`SXT5227E` | Cannot convert OPAQUE to IPPORT16
Explanation: Conversion of `OPAQUE` to `IPPORT16` has failed. User Response: Correct the recipe definition. System Action: The Input field is not processed.
`SXT5228E` | Cannot convert OPAQUE to IPADDR32
Explanation: Conversion of `OPAQUE` to `IPADDR32` has failed. User Response: Correct the recipe definition. System Action: The Input field is not processed.
`SXT5229E` | Cannot convert UNSIGN-PACK to IPADDR32
Explanation: Conversion from Unsigned Packed to `IPADDR32` is not supported. User Response: Correct the conversion rule. System Action: The conversion is marked as error.
`SXT5230E` | Cannot convert UNSIGN-ZDEC to IPADDR32
Explanation: Conversion from Unsigned Packed to `IPADDR32` is not supported. User Response: Correct the conversion rule. System Action: The conversion is marked as error.
`SXT5231E` | OPAQUE cannot be zero length
Explanation: The source field in the buffer resolved to a zero length, which is not supported in an `OPAQUE` field type. User Response: Correct the conversion rule or data. System Action: The conversion is marked as error.
`SXT5306E` | Required and not found
Explanation: The field is defined in the recipe as required but is not in the input message. User Response: Review the recipe definition. System Action: The remainder of the fields in the message are processed and then the message is rejected.
`SXT5309E` | Required and not found
Explanation: The field is defined in the recipe as required but is not in the input message. User Response: Review the recipe definition. System Action: The remainder of the fields in the message are processed and then the message is rejected.
`SXT5319E` | Addfield failed
Explanation: While constructing an output message, a messaging API call failed. User Response: Contact TIBCO Support with the information on the error from the log and trace files. System Action: The field is not added to message.
`SXT5324E` | Field must be type RVMSG
Explanation: The recipe step defines the field as `RVMSG` but the input message field is of some other type. User Response: Review the recipe definition. System Action: Processing of the message terminates.
`SXT5325E` | SubMsg create failed
Explanation: While processing an output message with embedded submessages, a call to API Func to create a submessage failed. Func: `tibrvMsg_Create` for Rendezvous message, ``tibemsMapMsg_Create``, or `tibemsStreamMsg_Create` for EMS message User Response: Contact TIBCO Support with the information on the error from the log and trace files. System Action: Processing of the submessage terminates.
`SXT5328I` | For CICS: U-Trc(RR) UoW:uow-number Task:task-number Idx:idx-number TID:Token-Id For IMS: U-Trc(RR) UoW:number TID:Token-Id
Explanation: While processing an outbound back-end request/reply message, this message is produced if trigger trace level is 2 or greater. uow-number is the unit of work ID assigned to this message. task-number is the CICS task number generating the message. idx-number is the CICS request/reply slot being used. token-id is the value for tibss-envelope. User Response: Review the log for information on the request/reply process that might be of use for debugging. System Action: Processing continues.
`SXT5330E` | Invalid Optional Special field
Explanation: A special field defined in the recipe is not in the message. Though optional, that field is not a valid special field for input. User Response: Review the recipe definition. System Action: The remaining fields in the message are processed and then the message is rejected.
`SXT5333E` | SubMsg AddMsg failed
Explanation: While processing an output message with embedded sub-messages, a call to API Func for a sub-message failed. Func: `tibrvMsg_AddMsg` for Rendezvous message, `tibemsMapMsg_SetMapMsg`, `tibemsMapMsg_SetStreamMsg`, `tibemsStreamMsg_WriteMapMsg`, or `tibemsStreamMsg_WriteStreamMsg` functions for EMS message User Response: Contact TIBCO Support with the information on the error from the log and trace files. System Action: Processing of the submessage terminates.
`SXT5334W` | SubMsg Destroy failed
Explanation: While processing an output message with embedded submessages, the `tibrvMsg_Destroy` function for a submessage failed. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT5342E` | Invalid Optional Special field
Explanation: A Special field defined in the recipe is not in the message. Though optional, that field is not a valid special field for input. User Response: Review the recipe definition. System Action: The remaining fields in the message are processed and then the message is rejected.
`SXT5343E` | Invalid Attributes
Explanation: An input special field is not of the correct type or size. User Response: Review the recipe definition. System Action: The remaining fields in the message are processed and then the message is rejected.
`SXT5344E` | Special Field not for Input
Explanation: An input special field is not of the correct type or size. User Response: Review the recipe definition. System Action: The remaining fields in the message are processed and then the message is rejected.
`SXT5346E` | Special Field not for Input
Explanation: A special field that is defined in an input conversion cannot be an input field. User Response: Review the recipe definition. System Action: The remaining fields in the message are processed and then the message is rejected.
`SXT5347E` | Add Envelope failed
Explanation: While constructing an outbound message, the recipe requested the special field Envelope. Func failed. Func: `tibrvMsg_AddOpaque` for Rendezvous message, `tibemsMapMsg_SetBytes`, or `tibemsStreamMsg_WriteBytes` functions for EMS message User Response: Contact TIBCO Support with the information on the error from the log and trace files. System Action: The field is not added to the message.
`SXT5348E` | Add config id failed
Explanation: While constructing an outbound message, the recipe requested the special field config ID. Func failed. Func: `tibrvMsg_AddString` for Rendezvous message, `tibemsMapMsg_SetString`, or `tibemsStreamMsg_WriteString` functions for EMS message User Response: Contact TIBCO Support with the information on the error from the log and trace files. System Action: The field is not added to the message.
`SXT5349E` | Add SS-id failed
Explanation: While constructing an outbound message, the recipe requested the special field SS-id. Func failed. Func: `tibrvMsg_AddString` for Rendezvous message, `tibemsMapMsg_SetString`, or `tibemsStreamMsg_WriteString` functions for EMS message User Response: Contact TIBCO Support with the information on the error from the log and trace files. System Action: The field is not added to the message.
`SXT5350E` | Spec Fld not for output
Explanation: While constructing an outbound message, the recipe requested a Special field that cannot be used for output. User Response: Review the recipe or trigger definition. System Action: The field is not added to the message.
`SXT5351E` | Add Envelope by bit failed
Explanation: While constructing an outbound message, a bit setting requested the special field Envelope. Func failed. Func: `tibrvMsg_AddOpaque` for Rendezvous message, `tibemsMapMsg_SetBytes`, or `tibemsStreamMsg_WriteBytes` functions for EMS message User Response: Contact TIBCO Support with the information on the error from the log and trace files. System Action: The field is not added to the message.
`SXT5365E` | F-Name Input Bytes size size greater than buffer bufsize
Explanation: In an EMS Bytes message, the data included is larger than the receiving buffer. User Response: Correct the recipe or input message. System Response: Transaction is rejected with an error message.
`SXT5406E` | No destination for output
Explanation: While sending a response message, the reply failed and no response subject was specified. User Response: Specify one or more output destinations. System Action: This error is added to the error submessage. The entire response message is sent to the error subject, if specified.
`SXT5414E` | Msg_Detach failed
Explanation: The call to `tibrvMsg_Detach` has failed. User Response: Contact TIBCO Support. System Action: Processing of this message is terminated and responses are sent.
`SXT5416E` | No thread specific info found
Explanation: The call to `pthread_getspecific` has returned a `null` pointer. User Response: Contact TIBCO Support. System Action: Processing of this message is terminated and responses are sent.
`SXT5418E` | No open entry in UOW list
Explanation: No UOW entry is available to process with this message. User Response: Enlarge the UOW list or slow the pace of input. System Action: Processing of this message is terminated and responses are sent.
`SXT5423E` | Failure in UOW Storage request
Explanation: No user area is available to service this message. User Response: Contact TIBCO Support. System Action: Processing of this message is terminated and responses are sent.
`SXT5431E` | Backend interface: Applid not responding Rsn: RSN
Explanation: The nonzero return code RSN is sent to `QandDispatch_Work`. User Response: Contact TIBCO Support. System Action: Processing of this message is terminated and responses are sent.
`SXT5445E` | BES data size less than required CFGID data size
Explanation: During the processing of a trigger, the user data area in the COMMAREA was found to be smaller than the buffer size defined in the configuration file. User Response: Adjust the buffer sizes in the configuration file and ensure that `TRIG-MAXSIZE` in the CICS Interface parameters file is large enough. System Action: Processing of this message is terminated and responses are sent.
`SXT5464E` | BES RC RC rsn RSN Unknown failure
Explanation: The back-end processor has returned code RC with reason code RSN. User Response: Review the definition of the back-end processor. System Action: Processing of this message is terminated and responses are sent.
`SXT5476E` | Create Msg failed rc RC
Explanation: While processing a trigger, the call to Func failed with return code RC. Func: `tibrvMsg_Create` for Rendezvous message or `tibemsMapMsg_Create` for EMS message User Response: Contact TIBCO Support with the information on the error from the log and trace files. System Action: Processing of the trigger’s definition terminates.
`SXT5480E` | Create Msg failed rc RC
Explanation: The call to Func failed with return code RC. Func: `tibrvMsg_Create` for Rendezvous message or `tibemsMapMsg_Create` for EMS message User Response: Contact TIBCO Support with the information on the error from the log and trace files. System Action: Processing of this message is terminated and responses are sent.

Copyright © TIBCO Software Inc. All rights reserved.