# Operational Commands

The Monitor Utility has a z/OS console interface for assisting in the control of the Monitor execution and allowing continuous processing. The following table describes the console commands that control the execution of the RED State Monitor Utility.

RED State Monitor Control Command
Command | Description
--- | ---
SHUT or TERM | Terminates the execution of RED State Monitor Utility.
STATS,<URL> | Prints all current totals and statistics for the monitor URL.

Two examples are listed as follows:

- F monitor job name,SHUT or P monitor job name
- F monitor job name,STATS,URL

Given below is an example of the output of the STATS command with URL TIBSS.MSGS#YODA

    Stats command Url:'TIBSS.MSGS#YODA'
    LPAR:CAFE Job:C512WW3  Member:TIBSS.MSGS#YODA
    XCF Status     :Active    RED Status     :Active    Buffer OvrFlow :0
    Msgs Discarded :0         Msgs Expired   :0         Msgs Held      :0
    Buffer Size    :8460      Msgs > Buff Sz :0
    Msgs Received  :6         Largest Size(R):1084      Max Msg Occ    :0
    Msgs in Pool   :0         Pool Overflows :0         HWM Buffers    :1
    Msg Reply      :3         Msg Reply(SNC) :0         Msg SNC NAck   :0
    Req/Reply      :0         Req/Reply Fail :0         Msg RC4        :0
    SNC Sig(S)     :3         SNC Sig(R)     :0
    Mux Exec       :7         Mux Abend      :0         Mux Msg Lost   :0

For the field description of the output please refer to Field Descriptions for output of XTUV,STATS
Copyright © TIBCO Software Inc. All rights reserved.