# Sample Output for XTUV,REAL Command

The following is an example of the output generated by the XTUV,REAL command:

## XTUV,REAL

    11:10:51.384
      Receivers Active       : 1 <== #RED not running due to Abend Limit
      Receivers Busy         : 1
      Receivers started      : 1
      Messages In Queue      : 0
      High Water Mark (HWM)  : 0
      Message Receives       : 13
      Message Replies        : 0
      Message Errors         : 13
      Abends (count, limit)  : 7 of 5 <== Manual Intervention Required
      Trigger Messages Sent  : 11

## Field Descriptions for output of XTUV,REAL

Field | Description
--- | ---
Receivers Active | The current number #RED receiver transactions that are active. #RED receivers process messages destined for CICS and can run concurrently. The maximum number of #RED receivers can be controlled by the parameter CICS-MAIN-MAX in the RED interface.
Receivers Busy | Total number of #RED receiver transactions that have been in busy mode.
Receivers started | Total number of CICS Start transactions issued to execute concurrent receivers.
Messages In Queue | Current number of messages waiting in the RED pool that still need to be processed.
High Water Mark (HWM) | Highest count of messages that were waiting in the RED pool to be processed.
Messages Receives | The total number of messages received.
Messages Replies | The total number of replies sent if it is required.
Messages Errors | The total number of messages in error.
Abends (count, limit) | The total number of #RED transactions or user programs that abended. The maximum limit of abend allowable #RED restarts. The initial limit value is 5. Disconnect and connect your RED interface to have this abend count value reset.
Trigger Messages Sent | The total number of trigger messages sent.

Copyright © TIBCO Software Inc. All rights reserved.