# IMS Sysplex Environment

The following figure shows a sample configuration of Substation ES in an IMS Sysplex environment:

Interruption of transactional and event-driven processing usually takes less than 10 seconds during a Substation ES switchover, assuming that all the components to which Substation ES connects and with which Substation ES communicates are running and available for processing.

Copyright © TIBCO Software Inc. All rights reserved.