# Log Entries Panel

In the Log Entries panel, you can select a log or trace record written to the log or trace disk file.

## Panel Layout

    SXLP002---------------------- Log Entries ------------------------ Row 1 of 29
    Command ===>                                                   Scroll ==> PAGE

    Sel  Time      Type   Msg Id    RC  Rsn Message
    - ------------- ---- -------- ---- ---- --------------------------------------
      11:09:54.0919 154  SXG1600I    0    0 Log Agent Starting - Logging to TIBLOG
      11:09:54.1126 154  SXG1800I    0    0 Parameter Log Agent Starting - Logging
      11:09:54.4368 154  SXS1000I    0    0 Starting ~ TIBCO Substation (ES) for O
      11:09:54.4596 154  SXS1009I    0    0 Substation (ES) - Version 2.0.0
      11:09:54.7894 154  SXG2801I    0    0 Initialized ~ Substation ES - Admin &
      11:09:55.0454 154  SXG2800I    0    0 Starting ~ Substation ES - Transformer
      11:09:55.0479   0  SXT5717I    0    0 Trace level 1, 10 work threads; Cfg:TI
      11:09:55.2871 154  SXG2801I    0    0 Initialized ~ Substation ES - Transfor
      11:09:55.3874 154  SXG2800I    0    0 Starting ~ Substation ES - CICS Interf
      11:09:55.4673 154  SXC3000I    0    0 CICSTS4G - Connect IICICS to CICS Regi
      11:09:55.5539 154  SXC3001I    0    0 CICSTS4G - Connect IICICS to CICS Regi
      11:09:55.5590 154  SXG2801I    0    0 Initialized ~ Substation ES - CICS Int
      11:09:55.5950 156  SXC3400I    0    0 CICSTS4G - Started CICS EXCI Session (
      11:09:55.6130 156  SXC3400I    0    0 CICSTS4G - Started CICS EXCI Session (
      11:09:55.6352 154  SXG2800I    0    0 Starting ~ Substation ES - IMS Interfa
      11:09:55.6612 154  SXI4000I    0    0 A01IMSG - Connect IIIMS to IMS Region
      11:09:55.7283 154  SXI4001I    0    0 A01IMSG - Connect IIIMS to IMS Region
      11:09:55.7326 154  SXG2801I    0    0 Initialized ~ Substation ES - IMS Inte
      11:09:55.7336 154  SXS1001I    0    0 Initialized ~ Substation ES for IVP's
      11:09:55.8350 154  SXG1801I    0    0 Parameter Log closed
      11:09:55.8362 154  SXS2120I    0    0 (B) HiMark:0 Occ:1024 Incr:0 Curr:0
      11:09:55.8363 154  SXS2121I    0    0 (F) Stress Levels Strt:768 Slow:819 St
      11:09:55.8408 154  SXS2120I    0    0 (A) HiMark:410 Occ:1024 Incr:102 Curr:
      11:09:55.8504 154  SXG2806I    0    0 Activated ~ Substation ES - CICS Inter
      11:09:55.8521 154  SXG2806I    0    0 Activated ~ Substation ES - Transforme
      11:09:55.8525   0  SXT5036I    0    0 All transformer tasks are Good To Go
      11:09:55.8525 154  SXG2806I    0    0 Activated ~ Substation ES - Admin & Op
      11:09:55.8531 154  SXG2806I    0    0 Activated ~ Substation ES - IMS Interf
      11:09:55.8610 154  SXG2806I    0    0 Activated ~ Substation ES for IVP's
    ******************************* Bottom of data ********************************

## Field Description

The following table lists the fields in the Log Entries panel:

Field | Description
--- | ---
Sel | If you specify S or X in the input column, a panel with all the values that relate to the selected message is displayed. Valid selections: S and X.
Time | The time that this message was recorded by Substation ES LTA Agent.
Type | The internal message type code.
Msg Id | The message identifier.
RC | The return code associated with the message.
Rsn | The reason code associated with the message.
Message | The initial part of the message description. The entire message is available if you select the panel with all the values that relate to the selected message.

Copyright © TIBCO Software Inc. All rights reserved.