# Substation ES

Substation ES Log and Trace Agents can write recorded information directly to the IBM z/OS System Logger Stream.

To start logging information to the IBM z/OS System Logger Stream, execute the following additional tasks before starting Substation ES.

To see the detailed steps of the JCL, see Mainframe Logger Definition section.

Recipe Statistics Stream Messages

Record Message | Record Example
--- | ---
Entered Substation ES | SXT5469I IId:IESBR91 U-Trc(E) UoW:1411911514 Recipe:ABCD BES:REDI01, Dest:TIB.CICS.C.Request CorrId:yodas-correl-id
Entered ESB input Received message | SXT5468I IId:IESBR91 U-Trc(R) UoW:1411911514 Recipe:ABCD
Exited ESB input mapping work | SXT5465I IId:IESBR91 U-Trc(I) UoW:1411911514 BES:REDI01
Entered CICS interface worker | SXG1885I IId:REDI01 U-Trc(I) UoW:1411911514
Exited CICS | SXG1887I IId:REDI01 U-Trc(O) UoW:1411911514
Sent response | SXT5303I IId:IESBR91 U-Trc(O) UoW:1411911514 Dest:TIB.CICS.C.Reply

Trigger Statistics Stream Messages

Record Message | Record Example
--- | ---
Sent response | SXT5303I IId:IESBR91 U-Trc(T) UoW:1411911514 Dest:TIB.CICS.C.Reply

Copyright © TIBCO Software Inc. All rights reserved.